--C1L2 is Now_Floor_Disp:inst1|always0~52
C1L2_p1_out = !Reset & !En;
C1L2_or_out = C1L2_p1_out;
C1L2 = !(C1L2_or_out);


--D1_Direction_Disp_Row2[1] is Now_Direction_Disp:inst2|Direction_Disp_Row2[1]
D1_Direction_Disp_Row2[1]_p1_out = !D1_Direction_Disp_Row2[1] & D1_Direction_Disp_Row2[0] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2];
D1_Direction_Disp_Row2[1]_or_out = D1_Direction_Disp_Row2[1]_p1_out;
D1_Direction_Disp_Row2[1]_reg_input = D1_Direction_Disp_Row2[1]_or_out;
D1_Direction_Disp_Row2[1] = DFFE(D1_Direction_Disp_Row2[1]_reg_input, GLOBAL(Clock_1Hz), , , );


--C1L1 is Now_Floor_Disp:inst1|Now_Floor_Disp_Data[4]~100
C1L1_p1_out = !Now_Floor[1] & !Now_Floor[2] & !Reset & !En & Now_Floor[3];
C1L1_p2_out = Now_Floor[2] & !Reset & !En & !Now_Floor[3];
C1L1_p3_out = !Reset & !En & !Now_Floor[3] & Now_Floor[0];
C1L1_or_out = C1L1_p1_out # C1L1_p2_out # C1L1_p3_out;
C1L1 = C1L1_or_out;


--B1L7 is Slave_Floor_Select:inst|always0~46
B1L7_p1_out = !Down_Request & !Reset & !En;
B1L7_p2_out = Up_Request & !Reset & !En;
B1L7_or_out = B1L7_p1_out # B1L7_p2_out;
B1L7 = B1L7_or_out;


--D1_Direction_Disp_Row2[3] is Now_Direction_Disp:inst2|Direction_Disp_Row2[3]
D1_Direction_Disp_Row2[3]_p1_out = D1_Direction_Disp_Row2[0] & D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2];
D1_Direction_Disp_Row2[3]_or_out = D1_Direction_Disp_Row2[3]_p1_out;
D1_Direction_Disp_Row2[3]_reg_input = D1_Direction_Disp_Row2[3]_or_out;
D1_Direction_Disp_Row2[3] = DFFE(D1_Direction_Disp_Row2[3]_reg_input, GLOBAL(Clock_1Hz), , , );


--C1L3 is Now_Floor_Disp:inst1|reduce_or~1078
C1L3_p1_out = !Reset & !En & !Now_Floor[0] & !Now_Floor[3] & Now_Floor[1];
C1L3_p2_out = !Reset & !En & !Now_Floor[0] & Now_Floor[3] & !Now_Floor[1] & !Now_Floor[2];
C1L3_or_out = C1L3_p1_out # C1L3_p2_out;
C1L3 = C1L3_or_out;


--C1L4 is Now_Floor_Disp:inst1|reduce_or~1084
C1L4_p0_out = !Reset & !En & Now_Floor[2] & !Now_Floor[1] & !Now_Floor[3] & !Now_Floor[0];
C1L4_p1_out = !Reset & !En & !Now_Floor[2] & Now_Floor[1] & !Now_Floor[3];
C1L4_p2_out = !Reset & !En & !Now_Floor[2] & !Now_Floor[3] & Now_Floor[0];
C1L4_p3_out = !Reset & !En & Now_Floor[1] & !Now_Floor[3] & Now_Floor[0];
C1L4_p4_out = !Reset & !En & !Now_Floor[2] & !Now_Floor[1] & Now_Floor[3];
C1L4_or_out = C1L4_p0_out # C1L4_p1_out # C1L4_p2_out # C1L4_p3_out # C1L4_p4_out;
C1L4 = C1L4_or_out;


--C1L5 is Now_Floor_Disp:inst1|reduce_or~1089
C1L5_p1_out = !Reset & !En & !Now_Floor[3] & !Now_Floor[2] & Now_Floor[1];
C1L5_p2_out = !Reset & !En & !Now_Floor[3] & Now_Floor[2] & !Now_Floor[1] & Now_Floor[0];
C1L5_p3_out = !Reset & !En & !Now_Floor[3] & Now_Floor[1] & !Now_Floor[0];
C1L5_p4_out = !Reset & !En & Now_Floor[3] & !Now_Floor[2] & !Now_Floor[1] & !Now_Floor[0];
C1L5_or_out = C1L5_p1_out # C1L5_p2_out # C1L5_p3_out # C1L5_p4_out;
C1L5 = C1L5_or_out;


--C1L6 is Now_Floor_Disp:inst1|reduce_or~1093
C1L6_p1_out = !Now_Floor[0] & !Reset & !En & Now_Floor[2] & !Now_Floor[3];
C1L6_p2_out = !Reset & !En & !Now_Floor[2] & Now_Floor[3] & !Now_Floor[1];
C1L6_p3_out = !Reset & !En & Now_Floor[2] & !Now_Floor[3] & !Now_Floor[1];
C1L6_or_out = C1L6_p1_out # C1L6_p2_out # C1L6_p3_out;
C1L6 = C1L6_or_out;


--B1L2 is Slave_Floor_Select:inst|CNT2[4]~15
B1L2_p1_out = Down_Request & !Up_Request & !Reset & !En;
B1L2_p2_out = B1L2 & B1L6;
B1L2_p3_out = Down_Request & B1L2;
B1L2_or_out = B1L2_p1_out # B1L2_p2_out # B1L2_p3_out;
B1L2 = B1L2_or_out;


--B1L3 is Slave_Floor_Select:inst|Slave_Floor[0]~64
B1L3_p1_out = !Reset & !En & B1L2;
B1L3_or_out = B1L3_p1_out;
B1L3 = B1L3_or_out;


--B1L1 is Slave_Floor_Select:inst|CNT1[4]~15
B1L1_p1_out = Up_Request & B1L7;
B1L1_p2_out = !B1L7 & B1L1;
B1L1_p3_out = Up_Request & B1L1;
B1L1_or_out = B1L1_p1_out # B1L1_p2_out # B1L1_p3_out;
B1L1 = B1L1_or_out;


--D1_Direction_Disp_Row2[0] is Now_Direction_Disp:inst2|Direction_Disp_Row2[0]
D1_Direction_Disp_Row2[0]_p1_out = !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[0];
D1_Direction_Disp_Row2[0]_or_out = D1_Direction_Disp_Row2[0]_p1_out;
D1_Direction_Disp_Row2[0]_reg_input = D1_Direction_Disp_Row2[0]_or_out;
D1_Direction_Disp_Row2[0] = DFFE(D1_Direction_Disp_Row2[0]_reg_input, GLOBAL(Clock_1Hz), , , );


--B1L4 is Slave_Floor_Select:inst|Slave_Floor[3]~66
B1L4_p1_out = !Reset & !En & B1L1;
B1L4_or_out = B1L4_p1_out;
B1L4 = B1L4_or_out;


--C1L7 is Now_Floor_Disp:inst1|reduce_or~1097
C1L7_p1_out = Now_Floor[0] & !Reset & !En & !Now_Floor[3] & Now_Floor[2];
C1L7_p2_out = !Reset & !En & !Now_Floor[3] & Now_Floor[1];
C1L7_p3_out = !Reset & !En & Now_Floor[3] & !Now_Floor[2] & !Now_Floor[1];
C1L7_or_out = C1L7_p1_out # C1L7_p2_out # C1L7_p3_out;
C1L7 = C1L7_or_out;


--C1L8 is Now_Floor_Disp:inst1|reduce_or~1102
C1L8_p1_out = !Reset & !En & !Now_Floor[2] & Now_Floor[1] & !Now_Floor[3];
C1L8_p2_out = !Reset & !En & Now_Floor[1] & !Now_Floor[3] & !Now_Floor[0];
C1L8_p3_out = !Reset & !En & !Now_Floor[2] & !Now_Floor[1] & Now_Floor[3];
C1L8_p4_out = !Reset & !En & Now_Floor[2] & !Now_Floor[1] & !Now_Floor[3];
C1L8_or_out = C1L8_p1_out # C1L8_p2_out # C1L8_p3_out # C1L8_p4_out;
C1L8 = C1L8_or_out;


--B1L5 is Slave_Floor_Select:inst|Slave_Floor[4]~69
B1L5_p1_out = !Reset & !En & B1L2;
B1L5_p2_out = !Reset & !En & B1L1;
B1L5_or_out = B1L5_p1_out # B1L5_p2_out;
B1L5 = B1L5_or_out;


--D1_Direction_Disp_Row2[2] is Now_Direction_Disp:inst2|Direction_Disp_Row2[2]
D1_Direction_Disp_Row2[2]_p1_out = !D1_Direction_Disp_Row2[0] & D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2];
D1_Direction_Disp_Row2[2]_or_out = D1_Direction_Disp_Row2[2]_p1_out;
D1_Direction_Disp_Row2[2]_reg_input = D1_Direction_Disp_Row2[2]_or_out;
D1_Direction_Disp_Row2[2] = DFFE(D1_Direction_Disp_Row2[2]_reg_input, GLOBAL(Clock_1Hz), , , );


--D1_Direction_Disp_Row2[4] is Now_Direction_Disp:inst2|Direction_Disp_Row2[4]
D1_Direction_Disp_Row2[4]_p1_out = !D1_Direction_Disp_Row2[3] & D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[0];
D1_Direction_Disp_Row2[4]_or_out = D1_Direction_Disp_Row2[4]_p1_out;
D1_Direction_Disp_Row2[4]_reg_input = D1_Direction_Disp_Row2[4]_or_out;
D1_Direction_Disp_Row2[4] = DFFE(D1_Direction_Disp_Row2[4]_reg_input, GLOBAL(Clock_1Hz), , , );


--D1L5 is Now_Direction_Disp:inst2|Direction_Disp_Row1[6]$latch$en_or~301
D1L5_p0_out = !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2];
D1L5_p1_out = Now_Direction[0] & Now_Direction[1];
D1L5_p2_out = !Now_Direction[0] & !Now_Direction[1];
D1L5_or_out = D1L6 # D1L5_p0_out # D1L5_p1_out # D1L5_p2_out # En # Reset;
D1L5 = D1L5_or_out;


--D1L01 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1060
D1L01_p1_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & D1_Direction_Disp_Row2[0];
D1L01_p2_out = !Now_Direction[0] & !Now_Direction[1];
D1L01_p3_out = Now_Direction[0] & Now_Direction[1];
D1L01_or_out = D1L51 # En # D1L01_p1_out # D1L01_p2_out # D1L01_p3_out # Reset;
D1L01 = D1L01_or_out;


--D1L31 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1066
D1L31_p1_out = !D1_Direction_Disp_Row2[2] & D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0];
D1L31_p2_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0];
D1L31_p3_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & Now_Direction[1];
D1L31_p4_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & D1_Direction_Disp_Row2[0] & Now_Direction[1];
D1L31_or_out = D1L61 # En # D1L31_p1_out # D1L31_p2_out # D1L31_p3_out # D1L31_p4_out;
D1L31 = D1L31_or_out;


--D1L41 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1068
D1L41_p0_out = !Now_Direction[1] & !Now_Direction[0];
D1L41_p1_out = D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2] & Now_Direction[1];
D1L41_p2_out = Now_Direction[1] & Now_Direction[0];
D1L41_p3_out = !D1_Direction_Disp_Row2[1] & D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2];
D1L41_p4_out = !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & D1_Direction_Disp_Row2[0] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2];
D1L41_or_out = D1L71 # D1L41_p0_out # D1L41_p1_out # D1L41_p2_out # D1L41_p3_out # D1L41_p4_out;
D1L41 = D1L41_or_out;


--D1L11 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1062
D1L11_p0_out = !Now_Direction[0] & !Now_Direction[1];
D1L11_p1_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & Now_Direction[0];
D1L11_p2_out = Now_Direction[0] & Now_Direction[1];
D1L11_p3_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0];
D1L11_p4_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & D1_Direction_Disp_Row2[0];
D1L11_or_out = D1L81 # D1L11_p0_out # D1L11_p1_out # D1L11_p2_out # D1L11_p3_out # D1L11_p4_out;
D1L11 = D1L11_or_out;


--D1L21 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1064
D1L21_p0_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0];
D1L21_p1_out = Now_Direction[0] & !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & D1_Direction_Disp_Row2[0];
D1L21_p2_out = Now_Direction[0] & Now_Direction[1];
D1L21_p3_out = !Now_Direction[0] & !Now_Direction[1];
D1L21_p4_out = !D1_Direction_Disp_Row2[2] & D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0];
D1L21_or_out = D1L91 # D1L21_p0_out # D1L21_p1_out # D1L21_p2_out # D1L21_p3_out # D1L21_p4_out;
D1L21 = D1L21_or_out;


--D1L7 is Now_Direction_Disp:inst2|Direction_Disp_Row1[6]~1114
D1L7_p1_out = D1L01 & D1L5;
D1L7_p2_out = !D1L5 & D1L7;
D1L7_p3_out = D1L01 & D1L7;
D1L7_or_out = D1L7_p1_out # D1L7_p2_out # D1L7_p3_out;
D1L7 = D1L7_or_out;


--D1L4 is Now_Direction_Disp:inst2|Direction_Disp_Row1[5]~1118
D1L4_p1_out = D1L11 & D1L5;
D1L4_p2_out = !D1L5 & D1L4;
D1L4_p3_out = D1L11 & D1L4;
D1L4_or_out = D1L4_p1_out # D1L4_p2_out # D1L4_p3_out;
D1L4 = D1L4_or_out;


--D1L3 is Now_Direction_Disp:inst2|Direction_Disp_Row1[4]~1122
D1L3_p1_out = D1L21 & D1L5;
D1L3_p2_out = !D1L5 & D1L3;
D1L3_p3_out = D1L21 & D1L3;
D1L3_or_out = D1L3_p1_out # D1L3_p2_out # D1L3_p3_out;
D1L3 = D1L3_or_out;


--D1L2 is Now_Direction_Disp:inst2|Direction_Disp_Row1[2]~1126
D1L2_p1_out = D1L31 & D1L5;
D1L2_p2_out = !D1L5 & D1L2;
D1L2_p3_out = D1L31 & D1L2;
D1L2_or_out = D1L2_p1_out # D1L2_p2_out # D1L2_p3_out;
D1L2 = D1L2_or_out;


--D1L1 is Now_Direction_Disp:inst2|Direction_Disp_Row1[1]~1130
D1L1_p1_out = D1L41 & D1L5;
D1L1_p2_out = !D1L5 & D1L1;
D1L1_p3_out = D1L41 & D1L1;
D1L1_or_out = D1L1_p1_out # D1L1_p2_out # D1L1_p3_out;
D1L1 = D1L1_or_out;


--D1L8 is Now_Direction_Disp:inst2|Direction_Disp_Row1[6]~1132
D1L8_or_out = D1L7;
D1L8 = D1L8_or_out;


--D1L9 is Now_Direction_Disp:inst2|Direction_Disp_Row1[6]~1134
D1L9_or_out = D1L7;
D1L9 = D1L9_or_out;


--D1L6 is Now_Direction_Disp:inst2|Direction_Disp_Row1[6]$latch$en_or~320
D1L6_p1_out = !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & !D1_Direction_Disp_Row2[3] & D1_Direction_Disp_Row2[2];
D1L6_p2_out = D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2];
D1L6_p3_out = !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & D1_Direction_Disp_Row2[0] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2];
D1L6_p4_out = !D1_Direction_Disp_Row2[1] & D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2];
D1L6 = D1L6_p1_out # D1L6_p2_out # D1L6_p3_out # D1L6_p4_out;


--D1L51 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1136
D1L51_p1_out = !D1_Direction_Disp_Row2[2] & D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0];
D1L51_p2_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0];
D1L51_p3_out = !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0];
D1L51 = D1L51_p1_out # D1L51_p2_out # D1L51_p3_out;


--D1L61 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1140
D1L61_p1_out = Now_Direction[0] & Now_Direction[1];
D1L61_p2_out = !Now_Direction[0] & !Now_Direction[1];
D1L61 = D1L61_p1_out # D1L61_p2_out # Reset;


--D1L71 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1144
D1L71_p3_out = !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[2] & Now_Direction[1];
D1L71 = Reset # En # D1L71_p3_out;


--D1L81 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1148
D1L81_p3_out = !D1_Direction_Disp_Row2[2] & D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & !D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0] & Now_Direction[0];
D1L81 = Reset # En # D1L81_p3_out;


--D1L91 is Now_Direction_Disp:inst2|Direction_Disp_Row1~1152
D1L91_p3_out = Now_Direction[0] & !D1_Direction_Disp_Row2[2] & !D1_Direction_Disp_Row2[3] & !D1_Direction_Disp_Row2[1] & D1_Direction_Disp_Row2[4] & !D1_Direction_Disp_Row2[0];
D1L91 = Reset # En # D1L91_p3_out;


--~GND~0 is ~GND~0
~GND~0_or_out = GND;
~GND~0 = ~GND~0_or_out;


--~GND~1 is ~GND~1
~GND~1_or_out = GND;
~GND~1 = ~GND~1_or_out;


--B1L6 is Slave_Floor_Select:inst|always0~45sexp
B1L6 = EXP(!Up_Request & !Reset & !En);


--Reset is Reset
--operation mode is input

Reset = INPUT();


--En is En
--operation mode is input

En = INPUT();


--Now_Floor[3] is Now_Floor[3]
--operation mode is input

Now_Floor[3] = INPUT();


--Now_Floor[2] is Now_Floor[2]
--operation mode is input

Now_Floor[2] = INPUT();


--Now_Floor[1] is Now_Floor[1]
--operation mode is input

Now_Floor[1] = INPUT();


--Now_Floor[0] is Now_Floor[0]
--operation mode is input

Now_Floor[0] = INPUT();


--Clock_1Hz is Clock_1Hz
--operation mode is input

Clock_1Hz = INPUT();


--Now_Direction[1] is Now_Direction[1]
--operation mode is input

Now_Direction[1] = INPUT();


--Now_Direction[0] is Now_Direction[0]
--operation mode is input

Now_Direction[0] = INPUT();


--Up_Request is Up_Request
--operation mode is input

Up_Request = INPUT();


--Down_Request is Down_Request
--operation mode is input

Down_Request = INPUT();


--Slave_Floor[2] is Slave_Floor[2]
--operation mode is output

Slave_Floor[2] = OUTPUT(~GND~0);


--Slave_Floor[1] is Slave_Floor[1]
--operation mode is output

Slave_Floor[1] = OUTPUT(~GND~1);


--Now_Floor_Disp_Select is Now_Floor_Disp_Select
--operation mode is output

Now_Floor_Disp_Select = OUTPUT(C1L2);


--Direction_Disp_Row2[1] is Direction_Disp_Row2[1]
--operation mode is output

Direction_Disp_Row2[1] = OUTPUT(D1_Direction_Disp_Row2[1]);


--Now_Floor_Disp_Data[4] is Now_Floor_Disp_Data[4]
--operation mode is output

Now_Floor_Disp_Data[4] = OUTPUT(C1L1);


--Direction_Disp_Row2[3] is Direction_Disp_Row2[3]
--operation mode is output

Direction_Disp_Row2[3] = OUTPUT(D1_Direction_Disp_Row2[3]);


--Now_Floor_Disp_Data[2] is Now_Floor_Disp_Data[2]
--operation mode is output

Now_Floor_Disp_Data[2] = OUTPUT(C1L3);


--Now_Floor_Disp_Data[5] is Now_Floor_Disp_Data[5]
--operation mode is output

Now_Floor_Disp_Data[5] = OUTPUT(C1L4);


--Now_Floor_Disp_Data[3] is Now_Floor_Disp_Data[3]
--operation mode is output

Now_Floor_Disp_Data[3] = OUTPUT(C1L5);


--Now_Floor_Disp_Data[1] is Now_Floor_Disp_Data[1]
--operation mode is output

Now_Floor_Disp_Data[1] = OUTPUT(C1L6);


--Slave_Floor[0] is Slave_Floor[0]
--operation mode is output

Slave_Floor[0] = OUTPUT(B1L3);


--Direction_Disp_Row2[0] is Direction_Disp_Row2[0]
--operation mode is output

Direction_Disp_Row2[0] = OUTPUT(D1_Direction_Disp_Row2[0]);


--Now_Floor_Disp_Data[6] is Now_Floor_Disp_Data[6]
--operation mode is output

Now_Floor_Disp_Data[6] = OUTPUT(C1L7);


--Now_Floor_Disp_Data[0] is Now_Floor_Disp_Data[0]
--operation mode is output

Now_Floor_Disp_Data[0] = OUTPUT(C1L8);


--Slave_Floor[3] is Slave_Floor[3]
--operation mode is output

Slave_Floor[3] = OUTPUT(B1L4);


--Slave_Floor[4] is Slave_Floor[4]
--operation mode is output

Slave_Floor[4] = OUTPUT(B1L5);


--Direction_Disp_Row2[2] is Direction_Disp_Row2[2]
--operation mode is output

Direction_Disp_Row2[2] = OUTPUT(D1_Direction_Disp_Row2[2]);


--Direction_Disp_Row2[4] is Direction_Disp_Row2[4]
--operation mode is output

Direction_Disp_Row2[4] = OUTPUT(D1_Direction_Disp_Row2[4]);


--Direction_Disp_Row1[6] is Direction_Disp_Row1[6]
--operation mode is output

Direction_Disp_Row1[6] = OUTPUT(D1L7);


--Direction_Disp_Row1[5] is Direction_Disp_Row1[5]
--operation mode is output

Direction_Disp_Row1[5] = OUTPUT(D1L4);


--Direction_Disp_Row1[4] is Direction_Disp_Row1[4]
--operation mode is output

Direction_Disp_Row1[4] = OUTPUT(D1L3);


--Direction_Disp_Row1[2] is Direction_Disp_Row1[2]
--operation mode is output

Direction_Disp_Row1[2] = OUTPUT(D1L2);


--Direction_Disp_Row1[1] is Direction_Disp_Row1[1]
--operation mode is output

Direction_Disp_Row1[1] = OUTPUT(D1L1);


--Direction_Disp_Row1[3] is Direction_Disp_Row1[3]
--operation mode is output

Direction_Disp_Row1[3] = OUTPUT(D1L8);


--Direction_Disp_Row1[0] is Direction_Disp_Row1[0]
--operation mode is output

Direction_Disp_Row1[0] = OUTPUT(D1L9);


