--A1L12 is always0~42 at LC5
A1L12_p1_out = !Down_Request & !En & !Reset;
A1L12_p2_out = Up_Request & !En & !Reset;
A1L12_or_out = A1L12_p1_out # A1L12_p2_out;
A1L12 = A1L12_or_out;


--A1L2 is CNT2[4]~15 at LC4
A1L2_p1_out = Down_Request & !Up_Request & !En & !Reset;
A1L2_p2_out = A1L2 & A1L02;
A1L2_p3_out = Down_Request & A1L2;
A1L2_or_out = A1L2_p1_out # A1L2_p2_out # A1L2_p3_out;
A1L2 = A1L2_or_out;


--A1L21 is Slave_Floor~56 at LC1
A1L21_p1_out = A1L2 & !En & !Reset;
A1L21_or_out = A1L21_p1_out;
A1L21 = A1L21_or_out;


--A1L1 is CNT1[4]~15 at LC2
A1L1_p1_out = Up_Request & A1L12;
A1L1_p2_out = !A1L12 & A1L1;
A1L1_p3_out = Up_Request & A1L1;
A1L1_or_out = A1L1_p1_out # A1L1_p2_out # A1L1_p3_out;
A1L1 = A1L1_or_out;


--A1L31 is Slave_Floor~58 at LC3
A1L31_p1_out = A1L1 & !En & !Reset;
A1L31_or_out = A1L31_p1_out;
A1L31 = A1L31_or_out;


--A1L41 is Slave_Floor~61 at LC8
A1L41_p1_out = A1L2 & !En & !Reset;
A1L41_p2_out = !En & !Reset & A1L1;
A1L41_or_out = A1L41_p1_out # A1L41_p2_out;
A1L41 = A1L41_or_out;


--~GND~0 is ~GND~0 at LC9
~GND~0_or_out = GND;
~GND~0 = ~GND~0_or_out;


--~GND~1 is ~GND~1 at LC11
~GND~1_or_out = GND;
~GND~1 = ~GND~1_or_out;


--A1L02 is always0~41sexp at SEXP1
A1L02 = EXP(!Up_Request & !En & !Reset);


--Reset is Reset at PIN_34
--operation mode is input

Reset = INPUT();


--En is En at PIN_51
--operation mode is input

En = INPUT();


--Up_Request is Up_Request at PIN_81
--operation mode is input

Up_Request = INPUT();


--Down_Request is Down_Request at PIN_73
--operation mode is input

Down_Request = INPUT();


--Slave_Floor[2] is Slave_Floor[2] at PIN_8
--operation mode is output

Slave_Floor[2] = OUTPUT(~GND~0);


--Slave_Floor[1] is Slave_Floor[1] at PIN_5
--operation mode is output

Slave_Floor[1] = OUTPUT(~GND~1);


--Slave_Floor[0] is Slave_Floor[0] at PIN_11
--operation mode is output

Slave_Floor[0] = OUTPUT(A1L21);


--Slave_Floor[3] is Slave_Floor[3] at PIN_10
--operation mode is output

Slave_Floor[3] = OUTPUT(A1L31);


--Slave_Floor[4] is Slave_Floor[4] at PIN_9
--operation mode is output

Slave_Floor[4] = OUTPUT(A1L41);






