--------------------------------------------------------------------------------------
Timing Analyzer Summary
--------------------------------------------------------------------------------------

Type           : Worst-case tsu
Slack          : N/A
Required Time  : None
Actual Time    : 4.000 ns
From           : Reset
To             : main:inst3|Data_drive:b2v_inst|Adc_Conv
From Clock     : 
To Clock       : Clk_SCL
Failed Paths   : 0

Type           : Worst-case tco
Slack          : N/A
Required Time  : None
Actual Time    : 24.600 ns
From           : main:inst3|Data_Read:b2v_inst1|Data[13]
To             : Current_Adjust_Drive
From Clock     : Clk_SCL
To Clock       : 
Failed Paths   : 0

Type           : Worst-case tpd
Slack          : N/A
Required Time  : None
Actual Time    : 11.400 ns
From           : Position_Set[11]
To             : Position_Adjust_Drive
From Clock     : 
To Clock       : 
Failed Paths   : 0

Type           : Worst-case th
Slack          : N/A
Required Time  : None
Actual Time    : 8.900 ns
From           : AD7895_Data
To             : main:inst3|Data_Read:b2v_inst1|Data[8]
From Clock     : 
To Clock       : Clk_SCL
Failed Paths   : 0

Type           : Clock Setup: 'Clk_SCL'
Slack          : N/A
Required Time  : None
Actual Time    : 97.09 MHz ( period = 10.300 ns )
From           : main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0]
To             : main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1]
From Clock     : Clk_SCL
To Clock       : Clk_SCL
Failed Paths   : 0

Type           : Clock Setup: 'Rate_Measure_Ctrl'
Slack          : N/A
Required Time  : None
Actual Time    : 142.86 MHz ( period = 7.000 ns )
From           : Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]
To             : Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]
From Clock     : Rate_Measure_Ctrl
To Clock       : Rate_Measure_Ctrl
Failed Paths   : 0

Type           : Clock Setup: 'Rate_Pulse'
Slack          : N/A
Required Time  : None
Actual Time    : 142.86 MHz ( period = 7.000 ns )
From           : Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]
To             : Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]
From Clock     : Rate_Pulse
To Clock       : Rate_Pulse
Failed Paths   : 0

Type           : Total number of failed paths
Slack          : 
Required Time  : 
Actual Time    : 
From           : 
To             : 
From Clock     : 
To Clock       : 
Failed Paths   : 0

--------------------------------------------------------------------------------------

