--B1_dffs[0] is lpm_counter:counter_out_rtl_0|dffs[0]
B1_dffs[0]_reg_input = VCC;
B1_dffs[0] = TFFE(B1_dffs[0]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[1] is lpm_counter:counter_out_rtl_0|dffs[1]
B1_dffs[1]_or_out = !B1_dffs[0];
B1_dffs[1]_reg_input = !B1_dffs[1]_or_out;
B1_dffs[1] = TFFE(B1_dffs[1]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[2] is lpm_counter:counter_out_rtl_0|dffs[2]
B1_dffs[2]_p1_out = B1_dffs[1] & B1_dffs[0];
B1_dffs[2]_or_out = B1_dffs[2]_p1_out;
B1_dffs[2]_reg_input = B1_dffs[2]_or_out;
B1_dffs[2] = TFFE(B1_dffs[2]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[3] is lpm_counter:counter_out_rtl_0|dffs[3]
B1_dffs[3]_p1_out = B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[3]_or_out = B1_dffs[3]_p1_out;
B1_dffs[3]_reg_input = B1_dffs[3]_or_out;
B1_dffs[3] = TFFE(B1_dffs[3]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[4] is lpm_counter:counter_out_rtl_0|dffs[4]
B1_dffs[4]_p1_out = B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[4]_or_out = B1_dffs[4]_p1_out;
B1_dffs[4]_reg_input = B1_dffs[4]_or_out;
B1_dffs[4] = TFFE(B1_dffs[4]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[5] is lpm_counter:counter_out_rtl_0|dffs[5]
B1_dffs[5]_p1_out = B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[5]_or_out = B1_dffs[5]_p1_out;
B1_dffs[5]_reg_input = B1_dffs[5]_or_out;
B1_dffs[5] = TFFE(B1_dffs[5]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[6] is lpm_counter:counter_out_rtl_0|dffs[6]
B1_dffs[6]_p1_out = B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[6]_or_out = B1_dffs[6]_p1_out;
B1_dffs[6]_reg_input = B1_dffs[6]_or_out;
B1_dffs[6] = TFFE(B1_dffs[6]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[7] is lpm_counter:counter_out_rtl_0|dffs[7]
B1_dffs[7]_p1_out = B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[7]_or_out = B1_dffs[7]_p1_out;
B1_dffs[7]_reg_input = B1_dffs[7]_or_out;
B1_dffs[7] = TFFE(B1_dffs[7]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[8] is lpm_counter:counter_out_rtl_0|dffs[8]
B1_dffs[8]_p1_out = B1_dffs[7] & B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[8]_or_out = B1_dffs[8]_p1_out;
B1_dffs[8]_reg_input = B1_dffs[8]_or_out;
B1_dffs[8] = TFFE(B1_dffs[8]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[9] is lpm_counter:counter_out_rtl_0|dffs[9]
B1_dffs[9]_p1_out = B1_dffs[8] & B1_dffs[7] & B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[9]_or_out = B1_dffs[9]_p1_out;
B1_dffs[9]_reg_input = B1_dffs[9]_or_out;
B1_dffs[9] = TFFE(B1_dffs[9]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[10] is lpm_counter:counter_out_rtl_0|dffs[10]
B1_dffs[10]_p1_out = B1_dffs[9] & B1_dffs[8] & B1_dffs[7] & B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[10]_or_out = B1_dffs[10]_p1_out;
B1_dffs[10]_reg_input = B1_dffs[10]_or_out;
B1_dffs[10] = TFFE(B1_dffs[10]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[11] is lpm_counter:counter_out_rtl_0|dffs[11]
B1_dffs[11]_p1_out = B1_dffs[10] & B1_dffs[9] & B1_dffs[8] & B1_dffs[7] & B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[11]_or_out = B1_dffs[11]_p1_out;
B1_dffs[11]_reg_input = B1_dffs[11]_or_out;
B1_dffs[11] = TFFE(B1_dffs[11]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[12] is lpm_counter:counter_out_rtl_0|dffs[12]
B1_dffs[12]_p1_out = B1_dffs[11] & B1_dffs[10] & B1_dffs[9] & B1_dffs[8] & B1_dffs[7] & B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[12]_or_out = B1_dffs[12]_p1_out;
B1_dffs[12]_reg_input = B1_dffs[12]_or_out;
B1_dffs[12] = TFFE(B1_dffs[12]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[13] is lpm_counter:counter_out_rtl_0|dffs[13]
B1_dffs[13]_p1_out = B1_dffs[12] & B1_dffs[11] & B1_dffs[10] & B1_dffs[9] & B1_dffs[8] & B1_dffs[7] & B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[13]_or_out = B1_dffs[13]_p1_out;
B1_dffs[13]_reg_input = B1_dffs[13]_or_out;
B1_dffs[13] = TFFE(B1_dffs[13]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[14] is lpm_counter:counter_out_rtl_0|dffs[14]
B1_dffs[14]_p1_out = B1_dffs[13] & B1_dffs[12] & B1_dffs[11] & B1_dffs[10] & B1_dffs[9] & B1_dffs[8] & B1_dffs[7] & B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[14]_or_out = B1_dffs[14]_p1_out;
B1_dffs[14]_reg_input = B1_dffs[14]_or_out;
B1_dffs[14] = TFFE(B1_dffs[14]_reg_input, GLOBAL(Clk_65536Hz), , , );


--B1_dffs[15] is lpm_counter:counter_out_rtl_0|dffs[15]
B1_dffs[15]_p1_out = B1_dffs[14] & B1_dffs[13] & B1_dffs[12] & B1_dffs[11] & B1_dffs[10] & B1_dffs[9] & B1_dffs[8] & B1_dffs[7] & B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[15]_or_out = B1_dffs[15]_p1_out;
B1_dffs[15]_reg_input = B1_dffs[15]_or_out;
B1_dffs[15] = TFFE(B1_dffs[15]_reg_input, GLOBAL(Clk_65536Hz), , , );


--Clk_65536Hz is Clk_65536Hz
--operation mode is input

Clk_65536Hz = INPUT();


--Reset is Reset
--operation mode is input

Reset = INPUT();


--counter_out[0] is counter_out[0]
--operation mode is output

counter_out[0] = OUTPUT(B1_dffs[0]);


--counter_out[1] is counter_out[1]
--operation mode is output

counter_out[1] = OUTPUT(B1_dffs[1]);


--counter_out[2] is counter_out[2]
--operation mode is output

counter_out[2] = OUTPUT(B1_dffs[2]);


--counter_out[3] is counter_out[3]
--operation mode is output

counter_out[3] = OUTPUT(B1_dffs[3]);


--counter_out[4] is counter_out[4]
--operation mode is output

counter_out[4] = OUTPUT(B1_dffs[4]);


--counter_out[5] is counter_out[5]
--operation mode is output

counter_out[5] = OUTPUT(B1_dffs[5]);


--counter_out[6] is counter_out[6]
--operation mode is output

counter_out[6] = OUTPUT(B1_dffs[6]);


--counter_out[7] is counter_out[7]
--operation mode is output

counter_out[7] = OUTPUT(B1_dffs[7]);


--counter_out[8] is counter_out[8]
--operation mode is output

counter_out[8] = OUTPUT(B1_dffs[8]);


--counter_out[9] is counter_out[9]
--operation mode is output

counter_out[9] = OUTPUT(B1_dffs[9]);


--counter_out[10] is counter_out[10]
--operation mode is output

counter_out[10] = OUTPUT(B1_dffs[10]);


--counter_out[11] is counter_out[11]
--operation mode is output

counter_out[11] = OUTPUT(B1_dffs[11]);


--counter_out[12] is counter_out[12]
--operation mode is output

counter_out[12] = OUTPUT(B1_dffs[12]);


--counter_out[13] is counter_out[13]
--operation mode is output

counter_out[13] = OUTPUT(B1_dffs[13]);


--counter_out[14] is counter_out[14]
--operation mode is output

counter_out[14] = OUTPUT(B1_dffs[14]);


--counter_out[15] is counter_out[15]
--operation mode is output

counter_out[15] = OUTPUT(B1_dffs[15]);


