--A1L18 is disp_select~923 at LC5
A1L18_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[5];
A1L18_p1_out = time_disp_select[5] & Stopwatch_EN;
A1L18_p2_out = time_disp_select[5] & Timepiece_EN;
A1L18_p3_out = time_disp_select[5] & TimeSet_EN;
A1L18_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[5] & Alarmclock_EN;
A1L18_or_out = A1L18_p0_out # A1L18_p1_out # A1L18_p2_out # A1L18_p3_out # A1L18_p4_out;
A1L18 = A1L18_or_out;


--A1L28 is disp_select~924 at LC7
A1L28_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[4];
A1L28_p1_out = time_disp_select[4] & Stopwatch_EN;
A1L28_p2_out = time_disp_select[4] & Timepiece_EN;
A1L28_p3_out = time_disp_select[4] & TimeSet_EN;
A1L28_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[4] & Alarmclock_EN;
A1L28_or_out = A1L28_p0_out # A1L28_p1_out # A1L28_p2_out # A1L28_p3_out # A1L28_p4_out;
A1L28 = A1L28_or_out;


--A1L38 is disp_select~925 at LC1
A1L38_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[3];
A1L38_p1_out = time_disp_select[3] & Stopwatch_EN;
A1L38_p2_out = time_disp_select[3] & Timepiece_EN;
A1L38_p3_out = time_disp_select[3] & TimeSet_EN;
A1L38_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[3] & Alarmclock_EN;
A1L38_or_out = A1L38_p0_out # A1L38_p1_out # A1L38_p2_out # A1L38_p3_out # A1L38_p4_out;
A1L38 = A1L38_or_out;


--A1L48 is disp_select~926 at LC3
A1L48_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[2];
A1L48_p1_out = time_disp_select[2] & Stopwatch_EN;
A1L48_p2_out = time_disp_select[2] & Timepiece_EN;
A1L48_p3_out = time_disp_select[2] & TimeSet_EN;
A1L48_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[2] & Alarmclock_EN;
A1L48_or_out = A1L48_p0_out # A1L48_p1_out # A1L48_p2_out # A1L48_p3_out # A1L48_p4_out;
A1L48 = A1L48_or_out;


--A1L58 is disp_select~927 at LC14
A1L58_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[1];
A1L58_p1_out = time_disp_select[1] & Stopwatch_EN;
A1L58_p2_out = time_disp_select[1] & Timepiece_EN;
A1L58_p3_out = time_disp_select[1] & TimeSet_EN;
A1L58_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[1] & Alarmclock_EN;
A1L58_or_out = A1L58_p0_out # A1L58_p1_out # A1L58_p2_out # A1L58_p3_out # A1L58_p4_out;
A1L58 = A1L58_or_out;


--A1L68 is disp_select~928 at LC13
A1L68_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[0];
A1L68_p1_out = time_disp_select[0] & Stopwatch_EN;
A1L68_p2_out = time_disp_select[0] & Timepiece_EN;
A1L68_p3_out = time_disp_select[0] & TimeSet_EN;
A1L68_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[0] & Alarmclock_EN;
A1L68_or_out = A1L68_p0_out # A1L68_p1_out # A1L68_p2_out # A1L68_p3_out # A1L68_p4_out;
A1L68 = A1L68_or_out;


--A1L01 is Data~2814 at SEXP18
A1L01 = EXP(!Stopwatch_EN & !Timepiece_EN & !TimeSet_EN);


--A1L6 is Data~2798 at LC21
A1L6_p0_out = A1L01 & time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & hour1[3];
A1L6_p1_out = A1L01 & second1[3] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0];
A1L6_p2_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute0[3];
A1L6_p3_out = A1L01 & !time_disp_select[5] & time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute1[3];
A1L6_p4_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & time_disp_select[4] & !time_disp_select[0] & hour0[3];
A1L6_or_out = A1L31 # A1L6_p0_out # A1L6_p1_out # A1L6_p2_out # A1L6_p3_out # A1L6_p4_out;
A1L6 = A1L6_or_out;


--A1L7 is Data~2800 at LC36
A1L7_p0_out = A1L32 & time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & hour1[0];
A1L7_p1_out = A1L32 & second1[0] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0];
A1L7_p2_out = A1L32 & !time_disp_select[5] & !time_disp_select[3] & time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute0[0];
A1L7_p3_out = A1L32 & !time_disp_select[5] & time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute1[0];
A1L7_p4_out = A1L32 & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & time_disp_select[4] & !time_disp_select[0] & hour0[0];
A1L7_or_out = A1L61 # A1L7_p0_out # A1L7_p1_out # A1L7_p2_out # A1L7_p3_out # A1L7_p4_out;
A1L7 = A1L7_or_out;


--A1L8 is Data~2802 at LC52
A1L8_p0_out = A1L42 & time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & hour1[2];
A1L8_p1_out = A1L42 & second1[2] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0];
A1L8_p2_out = A1L42 & !time_disp_select[5] & !time_disp_select[3] & time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute0[2];
A1L8_p3_out = A1L42 & !time_disp_select[5] & time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute1[2];
A1L8_p4_out = A1L42 & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & time_disp_select[4] & !time_disp_select[0] & hour0[2];
A1L8_or_out = A1L91 # A1L8_p0_out # A1L8_p1_out # A1L8_p2_out # A1L8_p3_out # A1L8_p4_out;
A1L8 = A1L8_or_out;


--A1L9 is Data~2804 at LC12
A1L9_p0_out = A1L52 & time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & hour1[1];
A1L9_p1_out = A1L52 & second1[1] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0];
A1L9_p2_out = A1L52 & !time_disp_select[5] & !time_disp_select[3] & time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute0[1];
A1L9_p3_out = A1L52 & !time_disp_select[5] & time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute1[1];
A1L9_p4_out = A1L52 & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & time_disp_select[4] & !time_disp_select[0] & hour0[1];
A1L9_or_out = A1L22 # A1L9_p0_out # A1L9_p1_out # A1L9_p2_out # A1L9_p3_out # A1L9_p4_out;
A1L9 = A1L9_or_out;


--A1L08 is disp_select[5]$latch~10 at LC72
A1L08_p1_out = A1L18 & A1L24;
A1L08_p2_out = A1L08 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L08_p3_out = A1L18 & A1L08;
A1L08_or_out = A1L08_p1_out # A1L08_p2_out # A1L08_p3_out;
A1L08 = A1L08_or_out;


--A1L87 is disp_select[4]$latch~10 at LC73
A1L87_p1_out = A1L28 & A1L24;
A1L87_p2_out = A1L87 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L87_p3_out = A1L28 & A1L87;
A1L87_or_out = A1L87_p1_out # A1L87_p2_out # A1L87_p3_out;
A1L87 = A1L87_or_out;


--A1L67 is disp_select[3]$latch~10 at LC78
A1L67_p1_out = A1L38 & A1L24;
A1L67_p2_out = A1L67 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L67_p3_out = A1L38 & A1L67;
A1L67_or_out = A1L67_p1_out # A1L67_p2_out # A1L67_p3_out;
A1L67 = A1L67_or_out;


--A1L47 is disp_select[2]$latch~10 at LC80
A1L47_p1_out = A1L48 & A1L24;
A1L47_p2_out = A1L47 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L47_p3_out = A1L48 & A1L47;
A1L47_or_out = A1L47_p1_out # A1L47_p2_out # A1L47_p3_out;
A1L47 = A1L47_or_out;


--A1L27 is disp_select[1]$latch~10 at LC77
A1L27_p1_out = A1L58 & A1L24;
A1L27_p2_out = A1L27 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L27_p3_out = A1L58 & A1L27;
A1L27_or_out = A1L27_p1_out # A1L27_p2_out # A1L27_p3_out;
A1L27 = A1L27_or_out;


--A1L07 is disp_select[0]$latch~10 at LC75
A1L07_p1_out = A1L68 & A1L24;
A1L07_p2_out = A1L07 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L07_p3_out = A1L68 & A1L07;
A1L07_or_out = A1L07_p1_out # A1L07_p2_out # A1L07_p3_out;
A1L07 = A1L07_or_out;


--A1L5 is Data[3]~2844 at LC71
A1L5_p1_out = A1L6 & A1L24;
A1L5_p2_out = A1L5 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L5_p3_out = A1L6 & A1L5;
A1L5_or_out = A1L5_p1_out # A1L5_p2_out # A1L5_p3_out;
A1L5 = A1L5_or_out;


--A1L2 is Data[0]~2848 at LC74
A1L2_p1_out = A1L7 & A1L24;
A1L2_p2_out = A1L2 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L2_p3_out = A1L7 & A1L2;
A1L2_or_out = A1L2_p1_out # A1L2_p2_out # A1L2_p3_out;
A1L2 = A1L2_or_out;


--A1L4 is Data[2]~2852 at LC79
A1L4_p1_out = A1L8 & A1L24;
A1L4_p2_out = A1L4 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L4_p3_out = A1L8 & A1L4;
A1L4_or_out = A1L4_p1_out # A1L4_p2_out # A1L4_p3_out;
A1L4 = A1L4_or_out;


--A1L3 is Data[1]~2856 at LC76
A1L3_p1_out = A1L9 & A1L24;
A1L3_p2_out = A1L3 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L3_p3_out = A1L9 & A1L3;
A1L3_or_out = A1L3_p1_out # A1L3_p2_out # A1L3_p3_out;
A1L3 = A1L3_or_out;


--A1L711 is reduce_or~1064 at LC65
A1L711_p1_out = A1L4 & !A1L3;
A1L711_p2_out = A1L3 & A1L5;
A1L711_or_out = A1L711_p1_out # A1L711_p2_out # A1L2;
A1L711 = !(A1L711_or_out);


--A1L811 is reduce_or~1070 at LC67
A1L811_p1_out = !A1L2 & !A1L4 & A1L3;
A1L811_p2_out = A1L4 & A1L5;
A1L811_p3_out = A1L3 & A1L5;
A1L811_or_out = A1L811_p1_out # A1L811_p2_out # A1L811_p3_out;
A1L811 = !(A1L811_or_out);


--A1L911 is reduce_or~1076 at LC69
A1L911_p1_out = A1L5 & A1L3;
A1L911_p2_out = A1L5 & A1L4;
A1L911_p3_out = !A1L3 & A1L4 & A1L2;
A1L911_p4_out = A1L3 & A1L4 & !A1L2;
A1L911_or_out = A1L911_p1_out # A1L911_p2_out # A1L911_p3_out # A1L911_p4_out;
A1L911 = !(A1L911_or_out);


--A1L021 is reduce_or~1082 at LC81
A1L021_p1_out = A1L2 & !A1L5 & !A1L4;
A1L021_p2_out = A1L5 & A1L4;
A1L021_p3_out = A1L2 & A1L3;
A1L021_p4_out = !A1L4 & A1L3;
A1L021_or_out = A1L021_p1_out # A1L021_p2_out # A1L021_p3_out # A1L021_p4_out;
A1L021 = !(A1L021_or_out);


--A1L121 is reduce_or~1088 at LC83
A1L121_p1_out = A1L5 & !A1L4 & !A1L3;
A1L121_p2_out = !A1L5 & !A1L4 & A1L3;
A1L121_p3_out = !A1L5 & A1L4 & !A1L2;
A1L121_p4_out = !A1L5 & A1L4 & !A1L3;
A1L121_or_out = A1L121_p1_out # A1L121_p2_out # A1L121_p3_out # A1L121_p4_out;
A1L121 = A1L121_or_out;


--A1L221 is reduce_or~1093 at LC70
A1L221_p1_out = A1L2 & A1L4 & !A1L5;
A1L221_p2_out = !A1L2 & !A1L4 & !A1L5;
A1L221_p3_out = !A1L4 & A1L5 & !A1L3;
A1L221_p4_out = !A1L5 & A1L3;
A1L221_or_out = A1L221_p1_out # A1L221_p2_out # A1L221_p3_out # A1L221_p4_out;
A1L221 = A1L221_or_out;


--A1L321 is reduce_or~1099 at LC85
A1L321_p0_out = A1L4 & A1L2 & A1L3;
A1L321_p1_out = A1L4 & !A1L2 & !A1L3;
A1L321_p2_out = !A1L4 & A1L2 & !A1L3 & !A1L5;
A1L321_p3_out = A1L3 & A1L5;
A1L321_p4_out = A1L4 & A1L5;
A1L321_or_out = A1L321_p0_out # A1L321_p1_out # A1L321_p2_out # A1L321_p3_out # A1L321_p4_out;
A1L321 = !(A1L321_or_out);


--A1L11 is Data~2858 at LC18
A1L11_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second0[3] & !TimeSet_EN;
A1L11_p2_out = Timepiece_EN & second0[3] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L11_p3_out = second0[3] & TimeSet_EN & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L11 = A1L11_p1_out # A1L11_p2_out # A1L11_p3_out;


--A1L21 is Data~2860 at LC19
A1L21_p0_out = alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour1[3];
A1L21_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second1[3] & !TimeSet_EN;
A1L21_p2_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute0[3];
A1L21_p3_out = !alarmclock_disp_select[5] & alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute1[3];
A1L21_p4_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour0[3];
A1L21 = A1L11 # A1L21_p0_out # A1L21_p1_out # A1L21_p2_out # A1L21_p3_out # A1L21_p4_out;


--A1L31 is Data~2866 at LC20
A1L31_p0_out = Stopwatch_EN & second0[3] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L31_p1_out = day0[3] & !Alarmclock_EN & !date_disp_select[5] & date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN;
A1L31_p2_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & day1[3];
A1L31_p3_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month0[3];
A1L31_p4_out = !Alarmclock_EN & date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month1[3];
A1L31 = A1L21 # A1L31_p0_out # A1L31_p1_out # A1L31_p2_out # A1L31_p3_out # A1L31_p4_out;


--A1L41 is Data~2872 at LC33
A1L41_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second0[0] & !TimeSet_EN;
A1L41_p2_out = Timepiece_EN & second0[0] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L41_p3_out = second0[0] & TimeSet_EN & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L41 = A1L41_p1_out # A1L41_p2_out # A1L41_p3_out;


--A1L51 is Data~2874 at LC34
A1L51_p0_out = alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour1[0];
A1L51_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second1[0] & !TimeSet_EN;
A1L51_p2_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute0[0];
A1L51_p3_out = !alarmclock_disp_select[5] & alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute1[0];
A1L51_p4_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour0[0];
A1L51 = A1L41 # A1L51_p0_out # A1L51_p1_out # A1L51_p2_out # A1L51_p3_out # A1L51_p4_out;


--A1L61 is Data~2880 at LC35
A1L61_p0_out = Stopwatch_EN & second0[0] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L61_p1_out = day0[0] & !Alarmclock_EN & !date_disp_select[5] & date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN;
A1L61_p2_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & day1[0];
A1L61_p3_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month0[0];
A1L61_p4_out = !Alarmclock_EN & date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month1[0];
A1L61 = A1L51 # A1L61_p0_out # A1L61_p1_out # A1L61_p2_out # A1L61_p3_out # A1L61_p4_out;


--A1L71 is Data~2886 at LC49
A1L71_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second0[2] & !TimeSet_EN;
A1L71_p2_out = Timepiece_EN & second0[2] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L71_p3_out = second0[2] & TimeSet_EN & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L71 = A1L71_p1_out # A1L71_p2_out # A1L71_p3_out;


--A1L81 is Data~2888 at LC50
A1L81_p0_out = alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour1[2];
A1L81_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second1[2] & !TimeSet_EN;
A1L81_p2_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute0[2];
A1L81_p3_out = !alarmclock_disp_select[5] & alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute1[2];
A1L81_p4_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour0[2];
A1L81 = A1L71 # A1L81_p0_out # A1L81_p1_out # A1L81_p2_out # A1L81_p3_out # A1L81_p4_out;


--A1L91 is Data~2894 at LC51
A1L91_p0_out = Stopwatch_EN & second0[2] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L91_p1_out = day0[2] & !Alarmclock_EN & !date_disp_select[5] & date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN;
A1L91_p2_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & day1[2];
A1L91_p3_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month0[2];
A1L91_p4_out = !Alarmclock_EN & date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month1[2];
A1L91 = A1L81 # A1L91_p0_out # A1L91_p1_out # A1L91_p2_out # A1L91_p3_out # A1L91_p4_out;


--A1L02 is Data~2900 at LC9
A1L02_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second0[1] & !TimeSet_EN;
A1L02_p2_out = Timepiece_EN & second0[1] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L02_p3_out = second0[1] & TimeSet_EN & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L02 = A1L02_p1_out # A1L02_p2_out # A1L02_p3_out;


--A1L12 is Data~2902 at LC10
A1L12_p0_out = alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour1[1];
A1L12_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second1[1] & !TimeSet_EN;
A1L12_p2_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute0[1];
A1L12_p3_out = !alarmclock_disp_select[5] & alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute1[1];
A1L12_p4_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour0[1];
A1L12 = A1L02 # A1L12_p0_out # A1L12_p1_out # A1L12_p2_out # A1L12_p3_out # A1L12_p4_out;


--A1L22 is Data~2908 at LC11
A1L22_p0_out = Stopwatch_EN & second0[1] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L22_p1_out = day0[1] & !Alarmclock_EN & !date_disp_select[5] & date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN;
A1L22_p2_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & day1[1];
A1L22_p3_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month0[1];
A1L22_p4_out = !Alarmclock_EN & date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month1[1];
A1L22 = A1L12 # A1L22_p0_out # A1L22_p1_out # A1L22_p2_out # A1L22_p3_out # A1L22_p4_out;


--A1L24 is always0~45sexp at SEXP65
A1L24 = EXP(!Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN);


--Timepiece_EN is Timepiece_EN at PIN_28
--operation mode is input

Timepiece_EN = INPUT();


--TimeSet_EN is TimeSet_EN at PIN_85
--operation mode is input

TimeSet_EN = INPUT();


--Stopwatch_EN is Stopwatch_EN at PIN_27
--operation mode is input

Stopwatch_EN = INPUT();


--time_disp_select[5] is time_disp_select[5] at PIN_22
--operation mode is input

time_disp_select[5] = INPUT();


--time_disp_select[4] is time_disp_select[4] at PIN_78
--operation mode is input

time_disp_select[4] = INPUT();


--time_disp_select[3] is time_disp_select[3] at PIN_9
--operation mode is input

time_disp_select[3] = INPUT();


--time_disp_select[2] is time_disp_select[2] at PIN_68
--operation mode is input

time_disp_select[2] = INPUT();


--time_disp_select[1] is time_disp_select[1] at PIN_79
--operation mode is input

time_disp_select[1] = INPUT();


--time_disp_select[0] is time_disp_select[0] at PIN_92
--operation mode is input

time_disp_select[0] = INPUT();


--Alarmclock_EN is Alarmclock_EN at PIN_61
--operation mode is input

Alarmclock_EN = INPUT();


--alarmclock_disp_select[5] is alarmclock_disp_select[5] at PIN_32
--operation mode is input

alarmclock_disp_select[5] = INPUT();


--alarmclock_disp_select[4] is alarmclock_disp_select[4] at PIN_98
--operation mode is input

alarmclock_disp_select[4] = INPUT();


--alarmclock_disp_select[3] is alarmclock_disp_select[3] at PIN_56
--operation mode is input

alarmclock_disp_select[3] = INPUT();


--alarmclock_disp_select[2] is alarmclock_disp_select[2] at PIN_69
--operation mode is input

alarmclock_disp_select[2] = INPUT();


--alarmclock_disp_select[1] is alarmclock_disp_select[1] at PIN_7
--operation mode is input

alarmclock_disp_select[1] = INPUT();


--alarmclock_disp_select[0] is alarmclock_disp_select[0] at PIN_83
--operation mode is input

alarmclock_disp_select[0] = INPUT();


--hour1[3] is hour1[3] at PIN_100
--operation mode is input

hour1[3] = INPUT();


--hour1[2] is hour1[2] at PIN_30
--operation mode is input

hour1[2] = INPUT();


--hour1[1] is hour1[1] at PIN_77
--operation mode is input

hour1[1] = INPUT();


--hour1[0] is hour1[0] at PIN_12
--operation mode is input

hour1[0] = INPUT();


--hour0[3] is hour0[3] at PIN_23
--operation mode is input

hour0[3] = INPUT();


--hour0[2] is hour0[2] at PIN_70
--operation mode is input

hour0[2] = INPUT();


--hour0[1] is hour0[1] at PIN_35
--operation mode is input

hour0[1] = INPUT();


--hour0[0] is hour0[0] at PIN_36
--operation mode is input

hour0[0] = INPUT();


--minute1[3] is minute1[3] at PIN_65
--operation mode is input

minute1[3] = INPUT();


--minute1[2] is minute1[2] at PIN_20
--operation mode is input

minute1[2] = INPUT();


--minute1[1] is minute1[1] at PIN_87
--operation mode is input

minute1[1] = INPUT();


--minute1[0] is minute1[0] at PIN_8
--operation mode is input

minute1[0] = INPUT();


--minute0[3] is minute0[3] at PIN_57
--operation mode is input

minute0[3] = INPUT();


--minute0[2] is minute0[2] at PIN_81
--operation mode is input

minute0[2] = INPUT();


--minute0[1] is minute0[1] at PIN_2
--operation mode is input

minute0[1] = INPUT();


--minute0[0] is minute0[0] at PIN_75
--operation mode is input

minute0[0] = INPUT();


--second1[3] is second1[3] at PIN_25
--operation mode is input

second1[3] = INPUT();


--second1[2] is second1[2] at PIN_14
--operation mode is input

second1[2] = INPUT();


--second1[1] is second1[1] at PIN_37
--operation mode is input

second1[1] = INPUT();


--second1[0] is second1[0] at PIN_88
--operation mode is input

second1[0] = INPUT();


--second0[3] is second0[3] at PIN_24
--operation mode is input

second0[3] = INPUT();


--second0[2] is second0[2] at PIN_1
--operation mode is input

second0[2] = INPUT();


--second0[1] is second0[1] at PIN_13
--operation mode is input

second0[1] = INPUT();


--second0[0] is second0[0] at PIN_76
--operation mode is input

second0[0] = INPUT();


--Date_EN is Date_EN at PIN_80
--operation mode is input

Date_EN = INPUT();


--DateSet_EN is DateSet_EN at PIN_6
--operation mode is input

DateSet_EN = INPUT();


--date_disp_select[5] is date_disp_select[5] at PIN_72
--operation mode is input

date_disp_select[5] = INPUT();


--date_disp_select[4] is date_disp_select[4] at PIN_94
--operation mode is input

date_disp_select[4] = INPUT();


--date_disp_select[3] is date_disp_select[3] at PIN_29
--operation mode is input

date_disp_select[3] = INPUT();


--date_disp_select[2] is date_disp_select[2] at PIN_17
--operation mode is input

date_disp_select[2] = INPUT();


--date_disp_select[1] is date_disp_select[1] at PIN_84
--operation mode is input

date_disp_select[1] = INPUT();


--date_disp_select[0] is date_disp_select[0] at PIN_5
--operation mode is input

date_disp_select[0] = INPUT();


--month1[3] is month1[3] at PIN_97
--operation mode is input

month1[3] = INPUT();


--month1[2] is month1[2] at PIN_33
--operation mode is input

month1[2] = INPUT();


--month1[1] is month1[1] at PIN_58
--operation mode is input

month1[1] = INPUT();


--month1[0] is month1[0] at PIN_19
--operation mode is input

month1[0] = INPUT();


--month0[3] is month0[3] at PIN_71
--operation mode is input

month0[3] = INPUT();


--month0[2] is month0[2] at PIN_55
--operation mode is input

month0[2] = INPUT();


--month0[1] is month0[1] at PIN_60
--operation mode is input

month0[1] = INPUT();


--month0[0] is month0[0] at PIN_93
--operation mode is input

month0[0] = INPUT();


--day1[3] is day1[3] at PIN_16
--operation mode is input

day1[3] = INPUT();


--day1[2] is day1[2] at PIN_21
--operation mode is input

day1[2] = INPUT();


--day1[1] is day1[1] at PIN_31
--operation mode is input

day1[1] = INPUT();


--day1[0] is day1[0] at PIN_96
--operation mode is input

day1[0] = INPUT();


--day0[3] is day0[3] at PIN_67
--operation mode is input

day0[3] = INPUT();


--day0[2] is day0[2] at PIN_64
--operation mode is input

day0[2] = INPUT();


--day0[1] is day0[1] at PIN_10
--operation mode is input

day0[1] = INPUT();


--day0[0] is day0[0] at PIN_99
--operation mode is input

day0[0] = INPUT();


--disp_select[5] is disp_select[5] at PIN_45
--operation mode is output

disp_select[5] = OUTPUT(A1L08);


--disp_select[4] is disp_select[4] at PIN_46
--operation mode is output

disp_select[4] = OUTPUT(A1L87);


--disp_select[3] is disp_select[3] at PIN_49
--operation mode is output

disp_select[3] = OUTPUT(A1L67);


--disp_select[2] is disp_select[2] at PIN_50
--operation mode is output

disp_select[2] = OUTPUT(A1L47);


--disp_select[1] is disp_select[1] at PIN_48
--operation mode is output

disp_select[1] = OUTPUT(A1L27);


--disp_select[0] is disp_select[0] at PIN_47
--operation mode is output

disp_select[0] = OUTPUT(A1L07);


--disp_data[2] is disp_data[2] at PIN_40
--operation mode is output

disp_data[2] = OUTPUT(A1L711);


--disp_data[4] is disp_data[4] at PIN_41
--operation mode is output

disp_data[4] = OUTPUT(A1L811);


--disp_data[5] is disp_data[5] at PIN_42
--operation mode is output

disp_data[5] = OUTPUT(A1L911);


--disp_data[6] is disp_data[6] at PIN_44
--operation mode is output

disp_data[6] = OUTPUT(A1L221);


--disp_data[1] is disp_data[1] at PIN_52
--operation mode is output

disp_data[1] = OUTPUT(A1L021);


--disp_data[0] is disp_data[0] at PIN_53
--operation mode is output

disp_data[0] = OUTPUT(A1L121);


--disp_data[3] is disp_data[3] at PIN_54
--operation mode is output

disp_data[3] = OUTPUT(A1L321);






--A1L32 is Data~2922 at SEXP33
A1L32 = EXP(!Stopwatch_EN & !Timepiece_EN & !TimeSet_EN);


--A1L42 is Data~2923 at SEXP49
A1L42 = EXP(!Stopwatch_EN & !Timepiece_EN & !TimeSet_EN);


--A1L52 is Data~2924 at SEXP9
A1L52 = EXP(!Stopwatch_EN & !Timepiece_EN & !TimeSet_EN);


