# -*- coding: mbcs -*-
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models.changeKey(fromName='Model-1', toName='coupling')
# Save by qq on Fri Dec 08 13:07:52 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models['coupling'].ConstrainedSketch(name='__profile__', sheetSize=0.2)
mdb.models['coupling'].sketches['__profile__'].sketchOptions.setValues(
    decimalPlaces=3)
mdb.models['coupling'].sketches['__profile__'].CircleByCenterPerimeter(center=(
    0.0, 0.0), point1=(0.05, 0.0))
mdb.models['coupling'].sketches['__profile__'].CircleByCenterPerimeter(center=(
    0.0, 0.0), point1=(0.02, 0.0))
mdb.models['coupling'].sketches['__profile__'].CircleByCenterPerimeter(center=(
    0.035, 0.0), point1=(0.04, 0.0))
mdb.models['coupling'].sketches['__profile__'].radialPattern(centerPoint=(0.0, 
    0.0), geomList=(mdb.models['coupling'].sketches['__profile__'].geometry[4], 
    ), number=6, totalAngle=360.0, vertexList=())
mdb.models['coupling'].Part(dimensionality=THREE_D, name='coupling1', type=
    DEFORMABLE_BODY)
mdb.models['coupling'].parts['coupling1'].BaseSolidExtrude(depth=0.02, sketch=
    mdb.models['coupling'].sketches['__profile__'])
del mdb.models['coupling'].sketches['__profile__']
# Save by qq on Fri Dec 08 13:10:37 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models['coupling'].ConstrainedSketch(name='__edit__', objectToCopy=
    mdb.models['coupling'].parts['coupling1'].features['Solid extrude-1'].sketch)
mdb.models['coupling'].parts['coupling1'].projectReferencesOntoSketch(filter=
    COPLANAR_EDGES, sketch=mdb.models['coupling'].sketches['__edit__'], 
    upToFeature=
    mdb.models['coupling'].parts['coupling1'].features['Solid extrude-1'])
del mdb.models['coupling'].sketches['__edit__']
mdb.models['coupling'].ConstrainedSketch(name='__edit__', objectToCopy=
    mdb.models['coupling'].parts['coupling1'].features['Solid extrude-1'].sketch)
mdb.models['coupling'].parts['coupling1'].projectReferencesOntoSketch(filter=
    COPLANAR_EDGES, sketch=mdb.models['coupling'].sketches['__edit__'], 
    upToFeature=
    mdb.models['coupling'].parts['coupling1'].features['Solid extrude-1'])
del mdb.models['coupling'].sketches['__edit__']
del mdb.models['coupling'].parts['coupling1']
mdb.models['coupling'].ConstrainedSketch(name='__profile__', sheetSize=0.2)
mdb.models['coupling'].sketches['__profile__'].sketchOptions.setValues(
    decimalPlaces=3)
mdb.models['coupling'].sketches['__profile__'].CircleByCenterPerimeter(center=(
    0.0, 0.0), point1=(0.05, 0.0))
mdb.models['coupling'].sketches['__profile__'].CircleByCenterPerimeter(center=(
    0.0, 0.0), point1=(0.02, 0.0))
mdb.models['coupling'].sketches['__profile__'].CircleByCenterPerimeter(center=(
    0.035, 0.0), point1=(0.04, 0.0))
mdb.models['coupling'].sketches['__profile__'].radialPattern(centerPoint=(0.0, 
    0.0), geomList=(mdb.models['coupling'].sketches['__profile__'].geometry[4], 
    ), number=6, totalAngle=360.0, vertexList=())
mdb.models['coupling'].Part(dimensionality=THREE_D, name='coupling1', type=
    DEFORMABLE_BODY)
mdb.models['coupling'].parts['coupling1'].BaseSolidExtrude(depth=0.02, sketch=
    mdb.models['coupling'].sketches['__profile__'])
del mdb.models['coupling'].sketches['__profile__']
mdb.models['coupling'].ConstrainedSketch(name='__profile__', sheetSize=0.2)
mdb.models['coupling'].sketches['__profile__'].sketchOptions.setValues(
    decimalPlaces=3)
mdb.models['coupling'].sketches['__profile__'].CircleByCenterPerimeter(center=(
    0.0, 0.0), point1=(0.02, 0.0))
mdb.models['coupling'].Part(dimensionality=THREE_D, name='coupling2', type=
    DEFORMABLE_BODY)
mdb.models['coupling'].parts['coupling2'].BaseSolidExtrude(depth=0.05, sketch=
    mdb.models['coupling'].sketches['__profile__'])
del mdb.models['coupling'].sketches['__profile__']
# Save by qq on Fri Dec 08 13:13:44 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models['coupling'].rootAssembly.DatumCsysByDefault(CARTESIAN)
mdb.models['coupling'].rootAssembly.Instance(dependent=ON, name='coupling1-1', 
    part=mdb.models['coupling'].parts['coupling1'])
mdb.models['coupling'].rootAssembly.Instance(dependent=ON, name='coupling2-1', 
    part=mdb.models['coupling'].parts['coupling2'])
mdb.models['coupling'].rootAssembly.translate(instanceList=('coupling2-1', ), 
    vector=(0.0, 0.0, 0.01))
# Save by qq on Fri Dec 08 13:15:06 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models['coupling'].rootAssembly.PartFromBooleanMerge(domain=GEOMETRY, 
    instances=(mdb.models['coupling'].rootAssembly.instances['coupling1-1'], 
    mdb.models['coupling'].rootAssembly.instances['coupling2-1']), name=
    'coupling')
mdb.models['coupling'].rootAssembly.Instance(dependent=ON, name='coupling-1', 
    part=mdb.models['coupling'].parts['coupling'])
mdb.models['coupling'].rootAssembly.suppressFeatures(('coupling1-1', 
    'coupling2-1'))
# Save by qq on Fri Dec 08 13:16:25 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
del mdb.models['coupling'].rootAssembly.features['coupling1-1']
del mdb.models['coupling'].rootAssembly.features['coupling2-1']
mdb.models['coupling'].rootAssembly.Instance(dependent=ON, name='coupling1-1', 
    part=mdb.models['coupling'].parts['coupling1'])
mdb.models['coupling'].rootAssembly.Instance(dependent=ON, name='coupling2-1', 
    part=mdb.models['coupling'].parts['coupling2'])
del mdb.models['coupling'].rootAssembly.features['coupling-1']
mdb.models['coupling'].rootAssembly.translate(instanceList=('coupling2-1', ), 
    vector=(0.0, 0.0, 0.01))
del mdb.models['coupling'].parts['coupling']
mdb.models['coupling'].rootAssembly.PartFromBooleanMerge(domain=GEOMETRY, 
    instances=(mdb.models['coupling'].rootAssembly.instances['coupling1-1'], 
    mdb.models['coupling'].rootAssembly.instances['coupling2-1']), name=
    'coupling')
mdb.models['coupling'].rootAssembly.Instance(dependent=ON, name='coupling-1', 
    part=mdb.models['coupling'].parts['coupling'])
mdb.models['coupling'].rootAssembly.suppressFeatures(('coupling1-1', 
    'coupling2-1'))
del mdb.models['coupling'].parts['coupling1']
del mdb.models['coupling'].parts['coupling2']
# Save by qq on Fri Dec 08 13:26:36 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
del mdb.models['coupling'].rootAssembly.features['coupling1-1']
del mdb.models['coupling'].rootAssembly.features['coupling2-1']
mdb.models['coupling'].Material(name='steel')
mdb.models['coupling'].materials['steel'].Density(table=((7800.0, ), ))
mdb.models['coupling'].materials['steel'].Elastic(table=((206000000000.0, 0.3), 
    ))
mdb.models['coupling'].HomogeneousSolidSection(material='steel', name=
    'Section-coupling', thickness=1.0)
mdb.models['coupling'].parts['coupling'].SectionAssignment(offset=0.0, region=
    Region(
    cells=mdb.models['coupling'].parts['coupling'].cells.getSequenceFromMask(
    mask=('[#1 ]', ), )), sectionName='Section-coupling')
# Save by qq on Fri Dec 08 13:27:48 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
del mdb.models['coupling'].sections['Section-coupling']
mdb.models['coupling'].HomogeneousSolidSection(material='steel', name=
    'Section-coupling', thickness=1.0)
del mdb.models['coupling'].parts['coupling'].sectionAssignments[0]
mdb.models['coupling'].parts['coupling'].SectionAssignment(offset=0.0, region=
    Region(
    cells=mdb.models['coupling'].parts['coupling'].cells.getSequenceFromMask(
    mask=('[#1 ]', ), )), sectionName='Section-coupling')
# Save by qq on Fri Dec 08 13:30:27 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models['coupling'].rootAssembly.regenerate()
mdb.models['coupling'].FrequencyStep(description='Modal analysis of a coupling'
    , name='Step-Modal', numEigen=30, previous='Initial')
# Save by qq on Fri Dec 08 13:33:55 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models['coupling'].DisplacementBC(amplitude=UNSET, createStepName=
    'Step-Modal', distributionType=UNIFORM, fixed=OFF, localCsys=None, name=
    'BC-1', region=Region(
    faces=mdb.models['coupling'].rootAssembly.instances['coupling-1'].faces.getSequenceFromMask(
    mask=('[#2 ]', ), )), u1=0.0, u2=0.0, u3=0.0, ur1=0.0, ur2=0.0, ur3=UNSET)
# Save by qq on Fri Dec 08 13:37:35 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models['coupling'].ZsymmBC(createStepName='Step-Modal', name='BC-2', 
    region=Region(
    faces=mdb.models['coupling'].rootAssembly.instances['coupling-1'].faces.getSequenceFromMask(
    mask=('[#1000 ]', ), )))
# Save by qq on Fri Dec 08 13:39:46 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models['coupling'].parts['coupling'].setMeshControls(elemShape=TET, 
    regions=mdb.models['coupling'].parts['coupling'].cells.getSequenceFromMask(
    ('[#1 ]', ), ), technique=FREE)
mdb.models['coupling'].parts['coupling'].seedPart(deviationFactor=0.05, size=
    0.0105)
mdb.models['coupling'].parts['coupling'].setElementType(elemTypes=(ElemType(
    elemCode=C3D8R, elemLibrary=STANDARD), ElemType(elemCode=C3D6, 
    elemLibrary=STANDARD), ElemType(elemCode=C3D4, elemLibrary=STANDARD, 
    distortionControl=DEFAULT)), regions=(
    mdb.models['coupling'].parts['coupling'].cells.getSequenceFromMask((
    '[#1 ]', ), ), ))
mdb.models['coupling'].parts['coupling'].generateMesh(boundaryPreview=ON)
mdb.models['coupling'].parts['coupling'].deleteMesh()
mdb.models['coupling'].parts['coupling'].seedPart(deviationFactor=0.05, size=
    0.005)
mdb.models['coupling'].parts['coupling'].setElementType(elemTypes=(ElemType(
    elemCode=C3D8R, elemLibrary=STANDARD), ElemType(elemCode=C3D6, 
    elemLibrary=STANDARD), ElemType(elemCode=C3D4, elemLibrary=STANDARD, 
    distortionControl=DEFAULT)), regions=(
    mdb.models['coupling'].parts['coupling'].cells.getSequenceFromMask((
    '[#1 ]', ), ), ))
mdb.models['coupling'].parts['coupling'].generateMesh(boundaryPreview=ON)
mdb.models['coupling'].parts['coupling'].generateMesh()
# Save by qq on Fri Dec 08 13:46:55 2006
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.models['coupling'].rootAssembly.regenerate()
mdb.Job(contactPrint=OFF, description='Frequency analysis of a coupling', 
    echoPrint=OFF, explicitPrecision=SINGLE, historyPrint=OFF, model='coupling'
    , modelPrint=OFF, multiprocessingMode=DEFAULT, name='coupling', 
    nodalOutputPrecision=SINGLE, numCpus=1, numDomains=1, 
    parallelizationMethodExplicit=DOMAIN, preMemory=2048.0, scratch='', 
    standardMemory=2048.0, standardMemoryPolicy=MODERATE, type=ANALYSIS, 
    userSubroutine='')
mdb.jobs['coupling'].submit(consistencyChecking=OFF)
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(STARTED, {'phase': BATCHPRE_PHASE, 
    'clientHost': 'little', 'handle': 2812, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(HEADING, {'phase': BATCHPRE_PHASE, 
    'heading': 'Frequency analysis of a coupling', 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(WARNING, {'phase': BATCHPRE_PHASE, 
    'message': 'THE BIAS PARAMETER HAS NO EFFECT AND WILL BE IGNORED SINCE THERE IS ONLY ONE FREQUENCY INTERVAL', 
    'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(WARNING, {'phase': BATCHPRE_PHASE, 
    'message': 'THE BIAS PARAMETER HAS NO EFFECT AND WILL BE IGNORED SINCE THERE IS ONLY ONE FREQUENCY INTERVAL', 
    'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(WARNING, {'phase': BATCHPRE_PHASE, 
    'message': 'DEGREE OF FREEDOM 4 IS NOT ACTIVE IN THIS MODEL AND CAN NOT BE RESTRAINED', 
    'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(WARNING, {'phase': BATCHPRE_PHASE, 
    'message': 'DEGREE OF FREEDOM 5 IS NOT ACTIVE IN THIS MODEL AND CAN NOT BE RESTRAINED', 
    'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FILE, {'phase': BATCHPRE_PHASE, 
    'file': 'G:\\ABAQUS\\coupling.odb', 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(COMPLETED, {'phase': BATCHPRE_PHASE, 
    'message': 'Analysis phase complete', 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(STARTED, {'phase': STANDARD_PHASE, 
    'clientHost': 'little', 'handle': 3380, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(STEP, {
    'stepName': 'Modal analysis of a coupling', 'phase': STANDARD_PHASE, 
    'stepId': 1, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 0, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(STATUS, {'totalTime': 0.0, 'attempts': 1, 
    'timeIncrement': 1e-36, 'increment': 0, 'stepTime': 0.0, 'step': 1, 
    'jobName': 'coupling', 'severe': 0, 'iterations': 0, 
    'phase': STANDARD_PHASE, 'equilibrium': 0})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 1, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 2, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 3, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 4, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 5, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 6, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 7, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 8, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 9, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 10, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 11, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 12, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 13, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 14, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 15, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 16, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 17, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 18, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 19, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 20, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 21, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 22, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 23, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 24, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 25, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 26, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 27, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 28, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 29, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(ODB_FRAME, {'phase': STANDARD_PHASE, 'step': 0, 
    'frame': 30, 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(STATUS, {'totalTime': 0.0, 'attempts': 1, 
    'timeIncrement': 1e-36, 'increment': 1, 'stepTime': 1e-36, 'step': 1, 
    'jobName': 'coupling', 'severe': 0, 'iterations': 0, 
    'phase': STANDARD_PHASE, 'equilibrium': 0})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(END_STEP, {'phase': STANDARD_PHASE, 'stepId': 1, 
    'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(COMPLETED, {'phase': STANDARD_PHASE, 
    'message': 'Analysis phase complete', 'jobName': 'coupling'})
mdb.jobs.has_key('coupling')
mdb.jobs['coupling']._Message(JOB_COMPLETED, {
    'time': 'Fri Dec 08 13:50:29 2006', 'jobName': 'coupling'})
# Save by qq on Fri Dec 08 14:15:42 2006
# Save by qq on Fri Dec 08 15:31:13 2006
