# -*- coding: mbcs -*-
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.ModelFromInputFile(inputFileName='C:/for book/chp14/static/forwater .inp', 
    name='forwater ')
mdb.models['forwater '].rootAssembly.instances['PART-1-1'].elements.getSequenceFromMask(
    mask=('[#8888:4 ]', ))
mdb.models['forwater '].rootAssembly.instances['PART-1-1'].elements.getSequenceFromMask(
    mask=('[#11110000:4 #1010000 ]', ))
mdb.models['forwater '].rootAssembly.Surface(face4Elements=
    mdb.models['forwater '].rootAssembly.instances['PART-1-1'].elements.getSequenceFromMask(
    mask=('[#8888:4 ]', ), ), face6Elements=
    mdb.models['forwater '].rootAssembly.instances['PART-1-1'].elements.getSequenceFromMask(
    mask=('[#11110000:4 #1010000 ]', ), ), name='LoadWater')
mdb.models['forwater '].Pressure(amplitude=UNSET, createStepName='Fill-1', 
    distributionType=HYDROSTATIC, field='', hZero=90.0, magnitude=900.0, name=
    'Load-11', region=
    mdb.models['forwater '].rootAssembly.surfaces['LoadWater'])
# Save by feamesh on Mon Jul 13 21:40:49 2009
from part import *
from material import *
from section import *
from assembly import *
from step import *
from interaction import *
from load import *
from mesh import *
from job import *
from sketch import *
from visualization import *
from connectorBehavior import *
mdb.Job(contactPrint=OFF, description='', echoPrint=OFF, explicitPrecision=
    SINGLE, historyPrint=OFF, model='forwater ', modelPrint=OFF, 
    multiprocessingMode=DEFAULT, name='test', nodalOutputPrecision=SINGLE, 
    numCpus=1, numDomains=1, parallelizationMethodExplicit=DOMAIN, preMemory=
    512.0, scratch='', standardMemory=512.0, standardMemoryPolicy=MODERATE, 
    type=ANALYSIS, userSubroutine='')
# Save by feamesh on Mon Jul 13 21:45:30 2009
